****** uart_led.vhd ******

  -- instantiate the LED controller
	LEDman: LED_manager PORT MAP(
		Channel_1_data 		=> rx_data,
		Channel_2_data 		=> gnd,
		Channel_1_enable 	=> rx_data_rdy,
		Channel_2_enable 	=> gnd(0),
		Selector 			=> sel_clk_rx,
		clock 				=> clk_rx,
		reset 				=> rst_clk_rx,
		data_out 			=> LED_o
	);


****** uart_led_simple_tb.vhd ******

	clk_pin <= not clk_pin after CLK_RX_PERIOD/2;
							
	rst_pin <= '1', '0' after CLK_RX_PERIOD*100;
			 
    sel_pin <= '0', '1' after 4.5 ms;

	UUT: uart_led 
		generic map (
		    CLOCK_RATE => CLOCK_RATE,	
            BAUD_RATE  =>  BAUD_RATE
        )
	    port map ( 
	        clk_pin      => clk_pin,
            rst_pin      => rst_pin,
            rxd_pin      => rxd_clk_rx,
            sel_pin      => sel_pin,
            led_pins     => led_pins
	    );