### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.
To see the actual file transmitted to Xilinx, please click here.

software_version_and_target_device
beta | FALSE | build_version | 2552052
date_generated | Thu Aug 22 14:47:10 2019 | os_platform | WIN64
product_version | Vivado v2019.1 (64-bit) | project_id | 96d90d29537e4f17843dcba61fad768f
project_iteration | 5 | random_id | 4e1236f89dbe59349eb2c24e5c011796
registration_id | 1_2_4_3 | route_design | TRUE
target_device | xcku040 | target_family | kintexu
target_package | ffva1156 | target_speed | -2
tool_flow | Vivado

user_environment
cpu_name | Intel(R) Xeon(R) E-2176M CPU @ 2.70GHz | cpu_speed | 2712 MHz
os_name | Windows Server 2016 or Windows 10 | os_release | major release (build 9200)
system_ram | 34.000 GB | total_processors | 1

vivado_usage

gui_handlers
basedialog_cancel=1 | basedialog_ok=15 | basedialog_yes=1 | exprunmenu_change_run_settings=4
exprunmenu_make_active=1 | expruntreepanel_exp_run_tree_table=9 | flownavigatortreepanel_flow_navigator_tree=2 | gettingstartedview_open_project=1
mainmenumgr_file=2 | mainmenumgr_project=1 | pacommandnames_close_project=1 | pacommandnames_run_bitgen=1
programoptionsdialog_report_strategy=2 | programoptionspanelimpl_strategy=4 | touchpointsurveydialog_remind_me_later=1

java_command_handlers
addsources=3 | autoconnecttarget=2 | closedesign=2 | closeproject=9
launchopentarget=1 | launchprogramfpga=3 | newproject=1 | openhardwaremanager=3
openproject=7 | projectsettingscmdhandler=1 | reportutilization=1 | runbitgen=6
runimplementation=2 | runsynthesis=1 | settopnode=1 | simulationclose=1
simulationrestart=1 | simulationrun=1 | simulationrunfortime=1 | toolssettings=1
viewtaskimplementation=1

other_data
guimode=10

project_data
constraintsetcount=1 | core_container=false | currentimplrun=impl_1 | currentsynthesisrun=synth_1
default_library=xil_defaultlib | designmode=RTL | export_simulation_activehdl=0 | export_simulation_ies=0
export_simulation_modelsim=0 | export_simulation_questa=0 | export_simulation_riviera=0 | export_simulation_vcs=0
export_simulation_xsim=0 | implstrategy=Vivado Implementation Defaults | launch_simulation_activehdl=0 | launch_simulation_ies=0
launch_simulation_modelsim=0 | launch_simulation_questa=0 | launch_simulation_riviera=0 | launch_simulation_vcs=0
launch_simulation_xsim=1 | simulator_language=Mixed | srcsetcount=6 | synthesisstrategy=Vivado Synthesis Defaults
target_language=VHDL | target_simulator=XSim | totalimplruns=1 | totalsynthesisruns=1

unisim_transformation
post_unisim_transformation
bufgce=1 | diffinbuf=1 | fdre=38 | fdse=6
gnd=3 | ibufctrl=3 | inbuf=2 | lut1=3
lut2=13 | lut3=6 | lut4=9 | lut5=9
lut6=14 | obuf=8 | vcc=6
pre_unisim_transformation
bufgce=1 | fdre=38 | fdse=6 | gnd=3
ibuf=2 | ibufds=1 | lut1=3 | lut2=13
lut3=6 | lut4=9 | lut5=9 | lut6=14
obuf=8 | vcc=6

synthesis
command_line_options
-assert=default::[not_specified] | -bufg=default::12 | -cascade_dsp=default::auto | -constrset=default::[not_specified]
-control_set_opt_threshold=default::auto | -directive=default::default | -fanout_limit=default::10000 | -flatten_hierarchy=default::rebuilt
-fsm_extraction=default::auto | -gated_clock_conversion=default::off | -generic=default::[not_specified] | -include_dirs=default::[not_specified]
-keep_equivalent_registers=default::[not_specified] | -max_bram=default::-1 | -max_bram_cascade_height=default::-1 | -max_dsp=default::-1
-max_uram=default::-1 | -max_uram_cascade_height=default::-1 | -mode=default::default | -name=default::[not_specified]
-no_lc=default::[not_specified] | -no_srlextract=default::[not_specified] | -no_timing_driven=default::[not_specified] | -part=xcku040-ffva1156-2-e
-resource_sharing=default::auto | -retiming=default::[not_specified] | -rtl=default::[not_specified] | -rtl_skip_constraints=default::[not_specified]
-rtl_skip_ip=default::[not_specified] | -seu_protect=default::none | -sfcu=default::[not_specified] | -shreg_min_size=default::3
-top=uart_led | -verilog_define=default::[not_specified]
usage
elapsed=00:00:28s | hls_ip=0 | memory_gain=1017.824MB | memory_peak=1397.676MB

xsim
command_line_options
-sim_mode=default::behavioral | -sim_type=default::